






**OSPF(Open Shortest Path First):**





Command For First Router




Command For Second Router



Assigning Static IP to the end devices:



**Output:**



Ping one device with another.